C2

c2#sh run

Building configuration...

Current configuration : 3173 bytes

!

! Last configuration change at 18:02:31 UTC Sat Jun 14 2025

!

version 15.6

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname c2

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

ethernet lmi ce

!

!

!

mmi polling-interval 60

no mmi auto-configure

no mmi pvc

mmi snmp-timeout 180

!

!

!

!

!

!

!

!

!

ip dhcp pool Cs2

network 10.1.2.0 255.255.255.0

default-router 10.1.2.1

!

!

!

ip cef

no ipv6 cef

!

multilink bundle-name authenticated

!

!

!

!

!

redundancy

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

interface Tunnel0

ip address 10.1.3.2 255.255.255.0

tunnel source GigabitEthernet0/1

tunnel destination 8.8.10.4

!

interface GigabitEthernet0/0

ip address 10.1.2.1 255.255.255.0

duplex auto

speed auto

media-type rj45

!

interface GigabitEthernet0/1

ip address dhcp

duplex auto

speed auto

media-type rj45

!

interface GigabitEthernet0/2

no ip address

shutdown

duplex auto

speed auto

media-type rj45

!

interface GigabitEthernet0/3

no ip address

shutdown

duplex auto

speed auto

media-type rj45

!

router ospf 100

network 10.1.0.0 0.0.255.255 area 0

!

ip forward-protocol nd

!

!

no ip http server

no ip http secure-server

!

!

!

!

control-plane