iSP1

ISP1#sh run

Building configuration...

Current configuration : 3389 bytes

!

version 15.6

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname ISP1

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

ethernet lmi ce

!

!

!

mmi polling-interval 60

no mmi auto-configure

no mmi pvc

mmi snmp-timeout 180

!

!

!

!

!

no ip icmp rate-limit unreachable

!

!

!

!

ip dhcp pool customer

network 8.8.10.0 255.255.255.0

default-router 8.8.10.1

dns-server 8.8.8.1

!

!

!

no ip domain lookup

ip cef

no ipv6 cef

!

multilink bundle-name authenticated

!

!

!

!

!

redundancy

!

no cdp log mismatch duplex

!

ip tcp synwait-time 5

!

!

!

!

!

!

!

!

!

!

!

!

!

interface GigabitEthernet0/0

ip address 8.8.10.1 255.255.255.0

duplex auto

speed auto

media-type rj45

!

interface GigabitEthernet0/1

ip address 8.8.8.2 255.255.255.0

duplex auto

speed auto

media-type rj45

!

interface GigabitEthernet0/2

no ip address

shutdown

duplex auto

speed auto

media-type rj45

!

interface GigabitEthernet0/3

no ip address

shutdown

duplex auto

speed auto

media-type rj45

!

router ospf 1

network 8.8.8.2 0.0.0.0 area 0

!

router bgp 65000

bgp log-neighbor-changes

redistribute connected

neighbor 8.8.8.1 remote-as 65000

neighbor 8.8.9.2 remote-as 65000

!

ip forward-protocol nd

!

!

no ip http server

no ip http secure-server

!

!

!

!

control-plane

!

!

line con 0

exec-timeout 0 0

privilege level 15

logging synchronous

line aux 0

exec-timeout 0 0

privilege level 15

logging synchronous

line vty 0 4

login

transport input none

!

no scheduler allocate

!

end